hdmi_controller_nios2_gen2_0 |

2024.03.04.17:42:34 | Datasheet

Overview

Processor
nios2_gen2_0 Nios II 19.1.0
All Components
nios2_gen2_0 altera_nios2_gen2 19.1.0
Memory Map

| nios2_gen2_0
data_master | instruction_master
nios2_gen2_0 |  |
debug_mem_slave |  |

## nios2_gen2_0

altera_nios2_gen2 v19.1.0

## Parameters
setting_showUnpublishedSettings | false
setting_showInternalSettings | false
setting_preciseIllegalMemAccessException | false
io_regionbase | 0
io_regionsize | 0
setting_support31bitdcachebypass | true
setting_activateTrace | false
mpu_useLimit | false
mpu_enabled | false
mmu_enabled | false
mmu_autoAssignTlbPtrSz | true
cpuReset | false
resetrequest_enabled | true
setting_shadowRegisterSets | 0
mpu_numOfInstRegion | 8
mpu_numOfDataRegion | 8
mmu_TLBMissExcOffset | 0
resetOffset | 0
exceptionOffset | 32
cpuID | 0
resetSlave | onchip_memory2.s1
mmu_TLBMissExcSlave | None
exceptionSlave | onchip_memory2.s1
setting_interruptControllerType | Internal
setting_branchpredictiontype | Dynamic
setting_bhtPtrSz | 8
mul_shift_choice | 0
mul_32_impl | 2
mul_64_impl | 0
shift_rot_impl | 1
dividerType | no_div
mpu_minInstRegionSize | 12
mpu_minDataRegionSize | 12
mmu_uitlbNumEntries | 4
mmu_udtlbNumEntries | 6
mmu_tlbPtrSz | 7
mmu_tlbNumWays | 16
mmu_processIDNumBits | 8
impl | Fast
icache_size | 4096
fa_cache_line | 2
fa_cache_linesize | 0
icache_numTCIM | 0
icache_burstType | None
dcache_bursts | false
dcache_victim_buf_impl | ram
dcache_size | 2048
dcache_numTCDM | 0
setting_ecc_present | false
debug_enabled | true
debug_debugReqSignals | false
debug_OCIOnchipTrace | _128
debug_hwbreakpoint | 0
debug_datatrigger | 0
debug_traceType | none
debug_traceStorage | onchip_trace
resetAbsoluteAddr | 262144
exceptionAbsoluteAddr | 262176
mmu_TLBMissExcAbsAddr | 0
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
BIG_ENDIAN | 0
BREAK_ADDR | 0x00080820
CPU_ARCH_NIOS2_R1 |
CPU_FREQ | 50000000u
CPU_ID_SIZE | 1
CPU_ID_VALUE | 0x00000000
CPU_IMPLEMENTATION | "fast"
DATA_ADDR_WIDTH | 20
DCACHE_BYPASS_MASK | 0x80000000
DCACHE_LINE_SIZE | 32
DCACHE_LINE_SIZE_LOG2 | 5
DCACHE_SIZE | 2048
EXCEPTION_ADDR | 0x00040020
FLASH_ACCELERATOR_LINES | 0
FLASH_ACCELERATOR_LINE_SIZE | 0
FLUSHDA_SUPPORTED |
HARDWARE_DIVIDE_PRESENT | 0
HARDWARE_MULTIPLY_PRESENT | 1
HARDWARE_MULX_PRESENT | 0
HAS_DEBUG_CORE | 1
HAS_DEBUG_STUB |
HAS_EXTRA_EXCEPTION_INFO |
HAS_ILLEGAL_INSTRUCTION_EXCEPTION |
HAS_JMPI_INSTRUCTION |
ICACHE_LINE_SIZE | 32
ICACHE_LINE_SIZE_LOG2 | 5
ICACHE_SIZE | 4096
INITDA_SUPPORTED |
INST_ADDR_WIDTH | 20
NUM_OF_SHADOW_REG_SETS | 0
OCI_VERSION | 1
RESET_ADDR | 0x00040000

generation took 0.00 seconds | rendering took 0.00 seconds