hdmi_controller_onchip_memory2 |

2024.03.04.17:42:33 | Datasheet

Overview

All Components
onchip_memory2 altera_avalon_onchip_memory2 19.3.8
Memory Map

onchip_memory2
s1

## onchip_memory2

altera_avalon_onchip_memory2 v19.3.8

## Parameters
allowInSystemMemoryContentEditor | true
blockType | AUTO
dataWidth | 32
dualPort | false
enableDiffWidth | false
initMemContent | true
initializationFileName | G:/Home/User/Desktop/ALCK/pin_verify/RTL/Daugther/HDMI-FMC_Terasic/svn_revC/A7SK_HDMI_FMC/software/HDMI_FMC/mem_init
enPRInitMode | false
instanceID | NONE
memorySize | 256000
readDuringWriteMode | DONT_CARE
singleClockOperation | false
slave1Latency | 1
slave2Latency | 1
useNonDefaultInitFile | false
useShallowMemBlocks | false
writable | true
ecc_enabled | false
resetrequest_enabled | true
generateLegacySim | false

## Software Assignments
ALLOW_IN_SYSTEM_MEMORY_CONTENT_EDITOR | 1
ALLOW_MRAM_SIM_CONTENTS_ONLY_FILE | 0
CONTENTS_INFO | ""
DUAL_PORT | 0
GUI_RAM_BLOCK_TYPE | AUTO
INIT_CONTENTS_FILE | hdmi_controller_onchip_memory2_onchip_memory2
INIT_MEM_CONTENT | 1
INSTANCE_ID | NONE
NON_DEFAULT_INIT_FILE_ENABLED | 0
RAM_BLOCK_TYPE | AUTO
READ_DURING_WRITE_MODE | DONT_CARE
SINGLE_CLOCK_OP | 0
SIZE_MULTIPLE | 1
SIZE_VALUE | 256000
WRITABLE | 1

generation took 0.00 seconds | rendering took 0.00 seconds