hdmi_controller_jtag_uart |

2024.03.04.17:42:31 | Datasheet

Overview

All Components
jtag_uart altera_avalon_jtag_uart 19.2.4
Memory Map

jtag_uart
avalon_jtag_slave

## jtag_uart

altera_avalon_jtag_uart v19.2.4

## Parameters
readBufferDepth | 64
readIRQThreshold | 8
useRegistersForReadBuffer | false
useRegistersForWriteBuffer | false
writeBufferDepth | 64
writeIRQThreshold | 8
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
READ_DEPTH | 64
READ_THRESHOLD | 8
WRITE_DEPTH | 64
WRITE_THRESHOLD | 8

generation took 0.00 seconds | rendering took 0.01 seconds