reconfig_iopll |

2024.03.04.17:43:48 | Datasheet

Overview

All Components
iopll_reconfig_0 altera_iopll_reconfig 19.4.0
Memory Map

iopll_reconfig_0
mgmt_avalon_slave

## iopll_reconfig_0

altera_iopll_reconfig v19.4.0

## Parameters
gui_device_family | Agilex 7
gui_advanced_reconfig | false
gui_cal_mode | false
gui_avalon_addr_width | 10
gui_reconfig_mif_filename | G:/joe/ACLK/svn/HDMI-FMC/A7SK_HDMI_FMC_revC/rec.mif
gui_wait_for_lock | true
gui_copy_mif | true
table_names | <html><b>General Information</b><br>,Number of IOPLL Configurations,Depth of MIF File,Width of MIF File,,<html><b>Configuration 0 parameters</b><br>,N_HIGH,N_BYPASS_EN,N_EVEN_DUTY_EN,N_LOW,M_HIGH,M_BYPASS_EN,M_SRC_MUX,M_EVEN_DUTY_EN,M_LOW,BANDWIDTH_CONTROL,RIPPLECAP,CHARGE_PUMP_CURRENT,C0_HIGH,C0_BYPASS_EN,C0_EVEN_DUTY_EN,C0_LOW,C1_HIGH,C1_BYPASS_EN,C1_EVEN_DUTY_EN,C1_LOW,C2_HIGH,C2_BYPASS_EN,C2_EVEN_DUTY_EN,C2_LOW,C3_HIGH,C3_BYPASS_EN,C3_EVEN_DUTY_EN,C3_LOW,C4_HIGH,C4_BYPASS_EN,C4_EVEN_DUTY_EN,C4_LOW,C5_HIGH,C5_BYPASS_EN,C5_EVEN_DUTY_EN,C5_LOW,C6_HIGH,C6_BYPASS_EN,C6_EVEN_DUTY_EN,C6_LOW,C7_HIGH,C7_BYPASS_EN,C7_EVEN_DUTY_EN,C7_LOW,C8_HIGH,C8_BYPASS_EN,C8_EVEN_DUTY_EN,C8_LOW,Configuration 0 size,Configuration 0 name
table_values | ,1,48,15,,,256,1,0,256,4,0,0,0,4,2,1,11,256,1,0,256,2,0,0,2,4,0,0,4,4,0,0,4,256,1,0,256,256,1,0,256,256,1,0,256,256,1,0,256,256,1,0,256,47,rec
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.00 seconds | rendering took 0.02 seconds