#============================================================
# Build by Terasic System Builder
#============================================================

set_global_assignment -name FAMILY "Cyclone V"
set_global_assignment -name DEVICE 5CEBA4F23C7
set_global_assignment -name TOP_LEVEL_ENTITY "DE0_CV_ADA"
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "14.0"
set_global_assignment -name LAST_QUARTUS_VERSION "14.0"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "13:31:36 NOVEMBER 12,2014"
set_global_assignment -name DEVICE_FILTER_PACKAGE FBGA
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 484
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 7

#============================================================
# CLOCK
#============================================================
set_location_assignment PIN_M9 -to CLOCK_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK_50
set_location_assignment PIN_H13 -to CLOCK2_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK2_50
set_location_assignment PIN_E10 -to CLOCK3_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK3_50
set_location_assignment PIN_V15 -to CLOCK4_50
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to CLOCK4_50

#============================================================
# SEG7
#============================================================
set_location_assignment PIN_U21 -to HEX0[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[0]
set_location_assignment PIN_V21 -to HEX0[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[1]
set_location_assignment PIN_W22 -to HEX0[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[2]
set_location_assignment PIN_W21 -to HEX0[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[3]
set_location_assignment PIN_Y22 -to HEX0[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[4]
set_location_assignment PIN_Y21 -to HEX0[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[5]
set_location_assignment PIN_AA22 -to HEX0[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX0[6]
set_location_assignment PIN_AA20 -to HEX1[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[0]
set_location_assignment PIN_AB20 -to HEX1[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[1]
set_location_assignment PIN_AA19 -to HEX1[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[2]
set_location_assignment PIN_AA18 -to HEX1[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[3]
set_location_assignment PIN_AB18 -to HEX1[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[4]
set_location_assignment PIN_AA17 -to HEX1[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[5]
set_location_assignment PIN_U22 -to HEX1[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX1[6]
set_location_assignment PIN_Y19 -to HEX2[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[0]
set_location_assignment PIN_AB17 -to HEX2[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[1]
set_location_assignment PIN_AA10 -to HEX2[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[2]
set_location_assignment PIN_Y14 -to HEX2[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[3]
set_location_assignment PIN_V14 -to HEX2[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[4]
set_location_assignment PIN_AB22 -to HEX2[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[5]
set_location_assignment PIN_AB21 -to HEX2[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX2[6]
set_location_assignment PIN_Y16 -to HEX3[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[0]
set_location_assignment PIN_W16 -to HEX3[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[1]
set_location_assignment PIN_Y17 -to HEX3[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[2]
set_location_assignment PIN_V16 -to HEX3[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[3]
set_location_assignment PIN_U17 -to HEX3[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[4]
set_location_assignment PIN_V18 -to HEX3[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[5]
set_location_assignment PIN_V19 -to HEX3[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX3[6]
set_location_assignment PIN_U20 -to HEX4[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[0]
set_location_assignment PIN_Y20 -to HEX4[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[1]
set_location_assignment PIN_V20 -to HEX4[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[2]
set_location_assignment PIN_U16 -to HEX4[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[3]
set_location_assignment PIN_U15 -to HEX4[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[4]
set_location_assignment PIN_Y15 -to HEX4[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[5]
set_location_assignment PIN_P9 -to HEX4[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX4[6]
set_location_assignment PIN_N9 -to HEX5[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[0]
set_location_assignment PIN_M8 -to HEX5[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[1]
set_location_assignment PIN_T14 -to HEX5[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[2]
set_location_assignment PIN_P14 -to HEX5[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[3]
set_location_assignment PIN_C1 -to HEX5[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[4]
set_location_assignment PIN_C2 -to HEX5[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[5]
set_location_assignment PIN_W19 -to HEX5[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to HEX5[6]

#============================================================
# KEY
#============================================================
set_location_assignment PIN_U7 -to KEY[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[0]
set_location_assignment PIN_W9 -to KEY[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[1]
set_location_assignment PIN_M7 -to KEY[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[2]
set_location_assignment PIN_M6 -to KEY[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to KEY[3]
set_location_assignment PIN_P22 -to RESET_N
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RESET_N

#============================================================
# LED
#============================================================
set_location_assignment PIN_AA2 -to LEDR[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[0]
set_location_assignment PIN_AA1 -to LEDR[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[1]
set_location_assignment PIN_W2 -to LEDR[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[2]
set_location_assignment PIN_Y3 -to LEDR[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[3]
set_location_assignment PIN_N2 -to LEDR[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[4]
set_location_assignment PIN_N1 -to LEDR[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[5]
set_location_assignment PIN_U2 -to LEDR[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[6]
set_location_assignment PIN_U1 -to LEDR[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[7]
set_location_assignment PIN_L2 -to LEDR[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[8]
set_location_assignment PIN_L1 -to LEDR[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to LEDR[9]

#============================================================
# microSD Card
#============================================================
set_location_assignment PIN_H11 -to SD_CLK
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_CLK
set_location_assignment PIN_B11 -to SD_CMD
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_CMD
set_location_assignment PIN_K9 -to SD_DATA[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_DATA[0]
set_location_assignment PIN_D12 -to SD_DATA[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_DATA[1]
set_location_assignment PIN_E12 -to SD_DATA[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_DATA[2]
set_location_assignment PIN_C11 -to SD_DATA[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD_DATA[3]

#============================================================
# SW
#============================================================
set_location_assignment PIN_U13 -to SW[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[0]
set_location_assignment PIN_V13 -to SW[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[1]
set_location_assignment PIN_T13 -to SW[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[2]
set_location_assignment PIN_T12 -to SW[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[3]
set_location_assignment PIN_AA15 -to SW[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[4]
set_location_assignment PIN_AB15 -to SW[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[5]
set_location_assignment PIN_AA14 -to SW[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[6]
set_location_assignment PIN_AA13 -to SW[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[7]
set_location_assignment PIN_AB13 -to SW[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[8]
set_location_assignment PIN_AB12 -to SW[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SW[9]

#============================================================
# VGA
#============================================================
set_location_assignment PIN_B6 -to VGA_B[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_B[0]
set_location_assignment PIN_B7 -to VGA_B[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_B[1]
set_location_assignment PIN_A8 -to VGA_B[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_B[2]
set_location_assignment PIN_A7 -to VGA_B[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_B[3]
set_location_assignment PIN_L7 -to VGA_G[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_G[0]
set_location_assignment PIN_K7 -to VGA_G[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_G[1]
set_location_assignment PIN_J7 -to VGA_G[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_G[2]
set_location_assignment PIN_J8 -to VGA_G[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_G[3]
set_location_assignment PIN_H8 -to VGA_HS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_HS
set_location_assignment PIN_A9 -to VGA_R[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_R[0]
set_location_assignment PIN_B10 -to VGA_R[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_R[1]
set_location_assignment PIN_C9 -to VGA_R[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_R[2]
set_location_assignment PIN_A5 -to VGA_R[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_R[3]
set_location_assignment PIN_G8 -to VGA_VS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to VGA_VS

#============================================================
# GPIO_0_1, GPIO_0_1 connect to ADA - High Speed ADC/DAC
#============================================================
set_location_assignment PIN_N16 -to ADC_OTR_A
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_OTR_A
set_location_assignment PIN_B16 -to ADC_DB[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[0]
set_location_assignment PIN_M16 -to ADC_OTR_B
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_OTR_B
set_location_assignment PIN_C16 -to ADC_DB[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[1]
set_location_assignment PIN_D17 -to ADC_DB[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[2]
set_location_assignment PIN_K20 -to ADC_DB[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[4]
set_location_assignment PIN_K21 -to ADC_DB[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[3]
set_location_assignment PIN_K22 -to ADC_DB[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[5]
set_location_assignment PIN_M20 -to ADC_DB[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[6]
set_location_assignment PIN_M21 -to ADC_DB[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[8]
set_location_assignment PIN_N21 -to ADC_DB[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[7]
set_location_assignment PIN_R22 -to ADC_DB[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[9]
set_location_assignment PIN_R21 -to ADC_DB[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[10]
set_location_assignment PIN_T22 -to ADC_DB[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[12]
set_location_assignment PIN_N20 -to ADC_DB[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[11]
set_location_assignment PIN_N19 -to ADC_DB[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DB[13]
set_location_assignment PIN_M22 -to ADC_CLK_A
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_CLK_A
set_location_assignment PIN_P19 -to ADC_DA[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[0]
set_location_assignment PIN_L22 -to ADC_CLK_B
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_CLK_B
set_location_assignment PIN_P17 -to ADC_DA[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[1]
set_location_assignment PIN_P16 -to ADC_DA[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[2]
set_location_assignment PIN_M18 -to ADC_DA[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[4]
set_location_assignment PIN_L18 -to ADC_DA[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[3]
set_location_assignment PIN_L17 -to ADC_DA[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[5]
set_location_assignment PIN_L19 -to ADC_DA[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[6]
set_location_assignment PIN_K17 -to ADC_DA[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[8]
set_location_assignment PIN_K19 -to ADC_DA[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[7]
set_location_assignment PIN_P18 -to ADC_DA[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[9]
set_location_assignment PIN_R15 -to ADC_DA[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[10]
set_location_assignment PIN_R17 -to ADC_DA[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[12]
set_location_assignment PIN_R16 -to ADC_DA[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[11]
set_location_assignment PIN_T20 -to ADC_DA[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_DA[13]
set_location_assignment PIN_T19 -to POWER_ON
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to POWER_ON
set_location_assignment PIN_T18 -to ADC_OEB_B
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_OEB_B
set_location_assignment PIN_T15 -to ADC_OEB_A
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC_OEB_A
set_location_assignment PIN_H16 -to SMA_DAC4
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SMA_DAC4
set_location_assignment PIN_A12 -to DAC_DA[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[13]
set_location_assignment PIN_H15 -to OSC_SMA_ADC4
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to OSC_SMA_ADC4
set_location_assignment PIN_B12 -to DAC_DA[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[12]
set_location_assignment PIN_A13 -to DAC_DA[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[11]
set_location_assignment PIN_B13 -to DAC_DA[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[9]
set_location_assignment PIN_C13 -to DAC_DA[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[10]
set_location_assignment PIN_D13 -to DAC_DA[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[8]
set_location_assignment PIN_G18 -to DAC_DA[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[7]
set_location_assignment PIN_G17 -to DAC_DA[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[5]
set_location_assignment PIN_H18 -to DAC_DA[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[6]
set_location_assignment PIN_J18 -to DAC_DA[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[4]
set_location_assignment PIN_J19 -to DAC_DA[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[3]
set_location_assignment PIN_G11 -to DAC_DA[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[1]
set_location_assignment PIN_H10 -to DAC_DA[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[2]
set_location_assignment PIN_J11 -to DAC_DA[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DA[0]
set_location_assignment PIN_H14 -to DAC_CLK_A
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_CLK_A
set_location_assignment PIN_A15 -to DAC_WRT_A
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_WRT_A
set_location_assignment PIN_J13 -to DAC_CLK_B
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_CLK_B
set_location_assignment PIN_L8 -to DAC_DB[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[13]
set_location_assignment PIN_B15 -to DAC_DB[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[12]
set_location_assignment PIN_C15 -to DAC_DB[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[11]
set_location_assignment PIN_E14 -to DAC_DB[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[9]
set_location_assignment PIN_E15 -to DAC_DB[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[10]
set_location_assignment PIN_E16 -to DAC_DB[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[8]
set_location_assignment PIN_F14 -to DAC_DB[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[5]
set_location_assignment PIN_F15 -to DAC_DB[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[7]
set_location_assignment PIN_F13 -to DAC_DB[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[4]
set_location_assignment PIN_F12 -to DAC_DB[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[6]
set_location_assignment PIN_G16 -to DAC_DB[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[1]
set_location_assignment PIN_G15 -to DAC_DB[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[3]
set_location_assignment PIN_G13 -to DAC_DB[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[0]
set_location_assignment PIN_G12 -to DAC_DB[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_DB[2]
set_location_assignment PIN_J17 -to DAC_WRT_B
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_WRT_B
set_location_assignment PIN_K16 -to DAC_MODE
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DAC_MODE

#============================================================
# End of pin assignments by Terasic System Builder
#============================================================


set_global_assignment -name ENABLE_SIGNALTAP ON
set_global_assignment -name USE_SIGNALTAP_FILE stp1_ADDA.stp
set_global_assignment -name SLD_NODE_CREATOR_ID 110 -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_ENTITY_NAME sld_signaltap -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_RAM_BLOCK_TYPE=AUTO" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_NODE_INFO=805334528" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_POWER_UP_TRIGGER=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STORAGE_QUALIFIER_INVERSION_MASK_LENGTH=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ATTRIBUTE_MEM_MODE=OFF" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_FLOW_USE_GENERATED=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_BITS=11" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_BUFFER_FULL_STOP=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_CURRENT_RESOURCE_WIDTH=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_IN_ENABLED=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ADVANCED_TRIGGER_ENTITY=basic,1," -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL_PIPELINE=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ENABLE_ADVANCED_TRIGGER=0" -section_id auto_signaltap_0
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name QIP_FILE V/lpm_pll.qip
set_global_assignment -name QIP_FILE V/lpm_nco10.qip
set_global_assignment -name QIP_FILE V/lpm_nco.qip
set_global_assignment -name QIP_FILE V/lpm_add.qip
set_global_assignment -name VERILOG_FILE V/C5G_ADDA.v
set_global_assignment -name SDC_FILE DE0_CV_ADA.SDC
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT trigger_in -to "ADDA_TEST:t|DAC_CLK_A" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SEGMENT_SIZE=4096" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SAMPLE_DEPTH=4096" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_clk -to "ADDA_TEST:t|SAMPLE_CLK" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[0] -to "ADDA_TEST:t|ADC_CLK_A" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[1] -to "ADDA_TEST:t|ADC_DA[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[2] -to "ADDA_TEST:t|ADC_DA[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[3] -to "ADDA_TEST:t|ADC_DA[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[4] -to "ADDA_TEST:t|ADC_DA[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[5] -to "ADDA_TEST:t|ADC_DA[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[6] -to "ADDA_TEST:t|ADC_DA[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[7] -to "ADDA_TEST:t|ADC_DA[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[8] -to "ADDA_TEST:t|ADC_DA[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[9] -to "ADDA_TEST:t|ADC_DA[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[10] -to "ADDA_TEST:t|ADC_DA[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[11] -to "ADDA_TEST:t|ADC_DA[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[12] -to "ADDA_TEST:t|ADC_DA[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[13] -to "ADDA_TEST:t|ADC_DA[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[14] -to "ADDA_TEST:t|ADC_DA[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[15] -to "ADDA_TEST:t|ADC_DB[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[16] -to "ADDA_TEST:t|ADC_DB[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[17] -to "ADDA_TEST:t|ADC_DB[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[18] -to "ADDA_TEST:t|ADC_DB[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[19] -to "ADDA_TEST:t|ADC_DB[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[20] -to "ADDA_TEST:t|ADC_DB[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[21] -to "ADDA_TEST:t|ADC_DB[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[22] -to "ADDA_TEST:t|ADC_DB[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[23] -to "ADDA_TEST:t|ADC_DB[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[24] -to "ADDA_TEST:t|ADC_DB[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[25] -to "ADDA_TEST:t|ADC_DB[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[26] -to "ADDA_TEST:t|ADC_DB[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[27] -to "ADDA_TEST:t|ADC_DB[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[28] -to "ADDA_TEST:t|ADC_DB[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[29] -to "ADDA_TEST:t|DAC_CLK_A" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[30] -to "ADDA_TEST:t|DAC_DA[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[31] -to "ADDA_TEST:t|DAC_DA[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[32] -to "ADDA_TEST:t|DAC_DA[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[33] -to "ADDA_TEST:t|DAC_DA[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[34] -to "ADDA_TEST:t|DAC_DA[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[35] -to "ADDA_TEST:t|DAC_DA[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[36] -to "ADDA_TEST:t|DAC_DA[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[37] -to "ADDA_TEST:t|DAC_DA[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[38] -to "ADDA_TEST:t|DAC_DA[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[39] -to "ADDA_TEST:t|DAC_DA[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[40] -to "ADDA_TEST:t|DAC_DA[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[41] -to "ADDA_TEST:t|DAC_DA[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[42] -to "ADDA_TEST:t|DAC_DA[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[43] -to "ADDA_TEST:t|DAC_DA[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[44] -to "ADDA_TEST:t|DAC_DB[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[45] -to "ADDA_TEST:t|DAC_DB[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[46] -to "ADDA_TEST:t|DAC_DB[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[47] -to "ADDA_TEST:t|DAC_DB[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[48] -to "ADDA_TEST:t|DAC_DB[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[49] -to "ADDA_TEST:t|DAC_DB[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[50] -to "ADDA_TEST:t|DAC_DB[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[51] -to "ADDA_TEST:t|DAC_DB[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[52] -to "ADDA_TEST:t|DAC_DB[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[53] -to "ADDA_TEST:t|DAC_DB[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[54] -to "ADDA_TEST:t|DAC_DB[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[55] -to "ADDA_TEST:t|DAC_DB[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[56] -to "ADDA_TEST:t|DAC_DB[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[57] -to "ADDA_TEST:t|DAC_DB[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[0] -to "ADDA_TEST:t|ADC_CLK_A" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[1] -to "ADDA_TEST:t|ADC_DA[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[2] -to "ADDA_TEST:t|ADC_DA[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[3] -to "ADDA_TEST:t|ADC_DA[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[4] -to "ADDA_TEST:t|ADC_DA[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[5] -to "ADDA_TEST:t|ADC_DA[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[6] -to "ADDA_TEST:t|ADC_DA[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[7] -to "ADDA_TEST:t|ADC_DA[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[8] -to "ADDA_TEST:t|ADC_DA[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[9] -to "ADDA_TEST:t|ADC_DA[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[10] -to "ADDA_TEST:t|ADC_DA[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[11] -to "ADDA_TEST:t|ADC_DA[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[12] -to "ADDA_TEST:t|ADC_DA[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[13] -to "ADDA_TEST:t|ADC_DA[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[14] -to "ADDA_TEST:t|ADC_DA[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[15] -to "ADDA_TEST:t|ADC_DB[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[16] -to "ADDA_TEST:t|ADC_DB[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[17] -to "ADDA_TEST:t|ADC_DB[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[18] -to "ADDA_TEST:t|ADC_DB[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[19] -to "ADDA_TEST:t|ADC_DB[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[20] -to "ADDA_TEST:t|ADC_DB[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[21] -to "ADDA_TEST:t|ADC_DB[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[22] -to "ADDA_TEST:t|ADC_DB[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[23] -to "ADDA_TEST:t|ADC_DB[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[24] -to "ADDA_TEST:t|ADC_DB[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[25] -to "ADDA_TEST:t|ADC_DB[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[26] -to "ADDA_TEST:t|ADC_DB[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[27] -to "ADDA_TEST:t|ADC_DB[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[28] -to "ADDA_TEST:t|ADC_DB[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[29] -to "ADDA_TEST:t|DAC_CLK_A" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[30] -to "ADDA_TEST:t|DAC_DA[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[31] -to "ADDA_TEST:t|DAC_DA[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[32] -to "ADDA_TEST:t|DAC_DA[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[33] -to "ADDA_TEST:t|DAC_DA[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[34] -to "ADDA_TEST:t|DAC_DA[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[35] -to "ADDA_TEST:t|DAC_DA[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[36] -to "ADDA_TEST:t|DAC_DA[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[37] -to "ADDA_TEST:t|DAC_DA[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[38] -to "ADDA_TEST:t|DAC_DA[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[39] -to "ADDA_TEST:t|DAC_DA[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[40] -to "ADDA_TEST:t|DAC_DA[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[41] -to "ADDA_TEST:t|DAC_DA[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[42] -to "ADDA_TEST:t|DAC_DA[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[43] -to "ADDA_TEST:t|DAC_DA[9]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[44] -to "ADDA_TEST:t|DAC_DB[0]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[45] -to "ADDA_TEST:t|DAC_DB[10]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[46] -to "ADDA_TEST:t|DAC_DB[11]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[47] -to "ADDA_TEST:t|DAC_DB[12]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[48] -to "ADDA_TEST:t|DAC_DB[13]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[49] -to "ADDA_TEST:t|DAC_DB[1]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[50] -to "ADDA_TEST:t|DAC_DB[2]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[51] -to "ADDA_TEST:t|DAC_DB[3]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[52] -to "ADDA_TEST:t|DAC_DB[4]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[53] -to "ADDA_TEST:t|DAC_DB[5]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[54] -to "ADDA_TEST:t|DAC_DB[6]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[55] -to "ADDA_TEST:t|DAC_DB[7]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[56] -to "ADDA_TEST:t|DAC_DB[8]" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[57] -to "ADDA_TEST:t|DAC_DB[9]" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_DATA_BITS=58" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_BITS=58" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK=00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK_LENGTH=200" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STORAGE_QUALIFIER_BITS=58" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INCREMENTAL_ROUTING=1" -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[0] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[1] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[2] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[3] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[4] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[5] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[6] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[7] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[8] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[9] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[10] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[11] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[12] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[13] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[14] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[15] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[16] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[17] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[18] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[19] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[20] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[21] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[22] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[23] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[24] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[25] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[26] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[27] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[28] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[29] -to auto_signaltap_0|vcc -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[30] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_instance_assignment -name POST_FIT_CONNECT_TO_SLD_NODE_ENTITY_PORT crc[31] -to auto_signaltap_0|gnd -section_id auto_signaltap_0
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top
set_global_assignment -name SLD_FILE db/stp1_ADDA_auto_stripped.stp