ADDRESS_ACLR_A=NONE
CLOCK_ENABLE_INPUT_A=BYPASS
CLOCK_ENABLE_OUTPUT_A=BYPASS
INIT_FILE=./vpg_source/gen_108.mif
INTENDED_DEVICE_FAMILY="Stratix III"
NUMWORDS_A=256
OPERATION_MODE=ROM
OUTDATA_ACLR_A=NONE
OUTDATA_REG_A=CLOCK0
WIDTHAD_A=8
WIDTH_A=1
WIDTH_BYTEENA_A=1
DEVICE_FAMILY="Stratix III"
address_a
clock0
rden_a
q_a
