<session jtag_chain="USB-Blaster [USB-0]" jtag_device="@1: EP4SGX230(.|ES) (0x024090DD)" sof_file="tr4_golden_top.sof">
  <display_tree gui_logging_enabled="0">
    <display_branch instance="auto_signaltap_0" log="USE_GLOBAL_TEMP" signal_set="USE_GLOBAL_TEMP" trigger="USE_GLOBAL_TEMP"/>
  </display_tree>
  <instance entity_name="sld_signaltap" is_auto_node="yes" is_expanded="true" name="auto_signaltap_0" source_file="sld_signaltap.vhd">
    <node_ip_info instance_id="0" mfg_id="110" node_id="0" version="6"/>
    <position_info>
      <single attribute="active tab" value="0"/>
      <single attribute="data horizontal scroll position" value="0"/>
      <single attribute="data vertical scroll position" value="0"/>
      <single attribute="zoom level denominator" value="1"/>
      <single attribute="zoom level numerator" value="1"/>
      <single attribute="zoom offset denominator" value="1"/>
      <single attribute="zoom offset numerator" value="130944"/>
    </position_info>
    <signal_set global_temp="1" name="signal_set: 2011/10/17 11:27:16  #0">
      <clock name="OSC_50_BANK1" polarity="posedge" tap_mode="classic"/>
      <config ram_type="M4K" reserved_data_nodes="0" reserved_storage_qualifier_nodes="0" reserved_trigger_nodes="0" sample_depth="128" trigger_in_enable="no" trigger_out_enable="no"/>
      <top_entity/>
      <signal_vec>
        <trigger_input_vec>
          <wire name="PCIE0_WAKE_n" tap_mode="classic" type="output pin"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[8]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[9]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|rx_verify_start" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|test_error" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|tx_pattern:tx_pat|error_insert" tap_mode="classic" type="combinatorial"/>
        </trigger_input_vec>
        <data_input_vec>
          <wire name="PCIE0_WAKE_n" tap_mode="classic" type="output pin"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[8]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[9]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|rx_verify_start" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|test_error" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|tx_pattern:tx_pat|error_insert" tap_mode="classic" type="combinatorial"/>
        </data_input_vec>
        <storage_qualifier_input_vec>
          <wire name="PCIE0_WAKE_n" tap_mode="classic" type="output pin"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[0]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[1]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[2]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[3]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[4]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[5]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[6]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[7]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[8]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[9]" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|rx_verify_start" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|rx_data_verify:rx_verify2|test_error" tap_mode="classic" type="combinatorial"/>
          <wire name="xcvr_test:g3|tx_pattern:tx_pat|error_insert" tap_mode="classic" type="combinatorial"/>
        </storage_qualifier_input_vec>
      </signal_vec>
      <presentation>
        <data_view>
          <net is_signal_inverted="no" name="xcvr_test:g3|tx_pattern:tx_pat|error_insert"/>
          <net is_signal_inverted="no" name="xcvr_test:g3|rx_data_verify:rx_verify2|test_error"/>
          <net is_signal_inverted="no" name="xcvr_test:g3|rx_data_verify:rx_verify2|rx_verify_start"/>
          <net is_signal_inverted="no" name="PCIE0_WAKE_n"/>
          <bus is_signal_inverted="no" link="all" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data" order="msb_to_lsb" radix="hex" state="collapse" type="combinatorial">
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[9]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[8]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[7]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[6]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[5]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[4]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[3]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[2]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[1]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[0]"/>
          </bus>
          <bus is_signal_inverted="no" link="all" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data" order="msb_to_lsb" radix="hex" state="collapse" type="combinatorial">
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[7]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[6]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[5]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[4]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[3]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[2]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[1]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[0]"/>
          </bus>
        </data_view>
        <setup_view>
          <net is_signal_inverted="no" name="xcvr_test:g3|tx_pattern:tx_pat|error_insert"/>
          <net is_signal_inverted="no" name="xcvr_test:g3|rx_data_verify:rx_verify2|test_error"/>
          <net is_signal_inverted="no" name="xcvr_test:g3|rx_data_verify:rx_verify2|rx_verify_start"/>
          <net is_signal_inverted="no" name="PCIE0_WAKE_n"/>
          <bus is_signal_inverted="no" link="all" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data" order="msb_to_lsb" radix="hex" state="collapse" type="combinatorial">
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[9]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[8]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[7]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[6]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[5]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[4]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[3]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[2]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[1]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|tx_pattern:tx_pat|tx_data[0]"/>
          </bus>
          <bus is_signal_inverted="no" link="all" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data" order="msb_to_lsb" radix="hex" state="collapse" type="combinatorial">
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[7]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[6]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[5]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[4]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[3]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[2]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[1]"/>
            <net is_signal_inverted="no" name="xcvr_test:g1|rx_data_verify:rx_verify|rx_data[0]"/>
          </bus>
        </setup_view>
      </presentation>
      <trigger CRC="58FC59C3" attribute_mem_mode="false" gap_record="true" global_temp="1" name="trigger: 2011/10/17 11:59:02  #0" position="pre" power_up_trigger_mode="false" record_data_gap="true" segment_size="1" storage_mode="off" storage_qualifier_disabled="no" storage_qualifier_port_is_pin="true" storage_qualifier_port_name="auto_stp_external_storage_qualifier" storage_qualifier_port_tap_mode="classic" trigger_in="dont_care" trigger_out="active high" trigger_type="circular">
        <power_up_trigger position="pre" storage_qualifier_disabled="no" trigger_in="dont_care" trigger_out="active high"/>
        <events use_custom_flow_control="no">
          <level enabled="yes" name="condition1" type="basic">'xcvr_test:g3|rx_data_verify:rx_verify2|test_error' == rising edge
            <power_up enabled="yes">
            </power_up>
            <op_node/>
          </level>
        </events>
        <storage_qualifier_events>
          <transitional>0000000000000000000000
            <pwr_up_transitional>0000000000000000000000</pwr_up_transitional>
          </transitional>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
          <storage_qualifier_level type="basic">
            <power_up>
            </power_up>
            <op_node/>
          </storage_qualifier_level>
        </storage_qualifier_events>
        <log>
          <data global_temp="1" name="log: 2011/10/17 11:59:17  #0" power_up_mode="false" sample_depth="128" trigger_position="16"> </data>
          <extradata>1111111111111111T111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111111</extradata>
        </log>
      </trigger>
    </signal_set>
  </instance>
  <mnemonics/>
  <static_plugin_mnemonics/>
  <global_info>
    <single attribute="active instance" value="0"/>
    <multi attribute="column width" size="23" value="34,34,381,74,68,70,88,88,98,98,88,88,110,101,101,101,101,101,101,101,101,107,78"/>
    <multi attribute="frame size" size="2" value="1566,797"/>
    <single attribute="jtag widget visible" value="1"/>
    <multi attribute="jtag widget size" size="2" value="398,120"/>
    <single attribute="instance widget visible" value="1"/>
    <single attribute="config widget visible" value="1"/>
    <single attribute="hierarchy widget visible" value="1"/>
    <single attribute="data log widget visible" value="1"/>
  </global_info>
</session>
