LPM_NUMWORDS=256
LPM_SHOWAHEAD=OFF
LPM_TYPE=dcfifo
LPM_WIDTH=32
LPM_WIDTHU=8
LPM_WIDTHU_R=9
LPM_WIDTH_R=16
OVERFLOW_CHECKING=ON
RDSYNC_DELAYPIPE=4
UNDERFLOW_CHECKING=ON
USE_EAB=ON
WRITE_ACLR_SYNCH=OFF
WRSYNC_DELAYPIPE=4
DEVICE_FAMILY="Cyclone IV E"
aclr
data
rdclk
rdreq
wrclk
wrreq
q
wrusedw
