# DE3 (DE3 Board) Configuration

## IO Group Power Configurations:

Configuration Table
IO Group | Voltage | Connector Type | Connector Description | Connect to | Board(s) on Bus
--- | --- | --- | --- | --- | ---
A | 3.3V | GPIO 0 and 1 | J13, GPIO 0/J14, GPIO 1 | -/- | -/-
B | 1.8V | DDR2 SODIMM | J9, DDR2 SO-DIMM | - | -
C | 3.3V | HSTC | J5 HSTC-C TOP/J6, HSTC-C BOTTOM | CLR(Camera Link Receiver)/- | CLR(Camera Link Receiver Board)
D | 3.3V | HSTC | J7, HSTC-D TOP | - | -

## Pin Assignments:

- CLOCK
- LED
- SEG7
- BUTTON
- SW (SLIDE SWITCH)
- DIP_SW (DIP SWITCH)
- MAX1619 (TEMPERATURE SENSOR)
- USB
- SDCARD
- GPIO0 (J13, GPIO 0)
- GPIO1 (J14, GPIO 1)
- DDR2 (J9, DDR2 SO-DIMM)
- HSTCC (J5 HSTC-C TOP/J6, HSTC-C BOTTOM)
- HSTCD (J7, HSTC-D TOP/J8, HSTC-D BOTTOM)

## Pin Assignment Table:

##

CLOCK
Name | Location | Direction | Standard
--- | --- | --- | ---
OSC_BA | AN18 | input | 3.3-V LVTTL
OSC_BB | AN16 | input | 1.8 V
OSC_BC | B17 | input | 3.3-V LVTTL
OSC_BD | B19 | input | 3.3-V LVTTL
OSC1_50 | T33 | input | 3.3-V LVTTL
OSC2_50 | W2 | input | 3.3-V LVTTL
CLK_OUT | V10 | output | 3.3-V LVTTL
EXT_CLK | U2 | input | 3.3-V LVTTL

##

LED
Name | Location | Direction | Standard
--- | --- | --- | ---
LEDR[0] | AD1 | output | 3.3-V LVTTL
LEDR[1] | AC1 | output | 3.3-V LVTTL
LEDR[2] | AC2 | output | 3.3-V LVTTL
LEDR[3] | AB2 | output | 3.3-V LVTTL
LEDR[4] | AC4 | output | 3.3-V LVTTL
LEDR[5] | AB4 | output | 3.3-V LVTTL
LEDR[6] | AA3 | output | 3.3-V LVTTL
LEDR[7] | AB3 | output | 3.3-V LVTTL
LEDG[0] | AB1 | output | 3.3-V LVTTL
LEDG[1] | AA1 | output | 3.3-V LVTTL
LEDG[2] | Y1 | output | 3.3-V LVTTL
LEDG[3] | Y2 | output | 3.3-V LVTTL
LEDG[4] | Y3 | output | 3.3-V LVTTL
LEDG[5] | W3 | output | 3.3-V LVTTL
LEDG[6] | AA4 | output | 3.3-V LVTTL
LEDG[7] | Y4 | output | 3.3-V LVTTL
LEDB[0] | AB5 | output | 3.3-V LVTTL
LEDB[1] | AB6 | output | 3.3-V LVTTL
LEDB[2] | AA6 | output | 3.3-V LVTTL
LEDB[3] | AA7 | output | 3.3-V LVTTL
LEDB[4] | Y7 | output | 3.3-V LVTTL
LEDB[5] | Y8 | output | 3.3-V LVTTL
LEDB[6] | Y9 | output | 3.3-V LVTTL
LEDB[7] | Y10 | output | 3.3-V LVTTL

##

SEG7
Name | Location | Direction | Standard
--- | --- | --- | ---
HEX0[0] | W12 | output | 3.3-V LVTTL
HEX0[1] | Y11 | output | 3.3-V LVTTL
HEX0[2] | W10 | output | 3.3-V LVTTL
HEX0[3] | W8 | output | 3.3-V LVTTL
HEX0[4] | W7 | output | 3.3-V LVTTL
HEX0[5] | Y5 | output | 3.3-V LVTTL
HEX0[6] | Y6 | output | 3.3-V LVTTL
HEX0_DP | V3 | output | 3.3-V LVTTL
HEX1[0] | P3 | output | 3.3-V LVTTL
HEX1[1] | N4 | output | 3.3-V LVTTL
HEX1[2] | N3 | output | 3.3-V LVTTL
HEX1[3] | N1 | output | 3.3-V LVTTL
HEX1[4] | M1 | output | 3.3-V LVTTL
HEX1[5] | L1 | output | 3.3-V LVTTL
HEX1[6] | L2 | output | 3.3-V LVTTL
HEX1_DP | V4 | output | 3.3-V LVTTL

##

BUTTON
Name | Location | Direction | Standard
--- | --- | --- | ---
Button[0] | K1 | input | 3.3-V LVTTL
Button[1] | K2 | input | 3.3-V LVTTL
Button[2] | M4 | input | 3.3-V LVTTL
Button[3] | M3 | input | 3.3-V LVTTL

##

SW (SLIDE SWITCH)
Name | Location | Direction | Standard
--- | --- | --- | ---
SW[0] | W5 | input | 3.3-V LVTTL
SW[1] | W6 | input | 3.3-V LVTTL
SW[2] | W9 | input | 3.3-V LVTTL
SW[3] | W11 | input | 3.3-V LVTTL

##

DIP_SW (DIP SWITCH)
Name | Location | Direction | Standard
--- | --- | --- | ---
DIP_SW[0] | R12 | input | 3.3-V LVTTL
DIP_SW[1] | P5 | input | 3.3-V LVTTL
DIP_SW[2] | R4 | input | 3.3-V LVTTL
DIP_SW[3] | R3 | input | 3.3-V LVTTL
DIP_SW[4] | P2 | input | 3.3-V LVTTL
DIP_SW[5] | R1 | input | 3.3-V LVTTL
DIP_SW[6] | T2 | input | 3.3-V LVTTL
DIP_SW[7] | T1 | input | 3.3-V LVTTL

##

MAX1619 (TEMPERATURE SENSOR)
Name | Location | Direction | Standard
--- | --- | --- | ---
TEMP_CLK | P4 | output | 3.3-V LVTTL
TEMP_DATA | P1 | inout | 3.3-V LVTTL
TEMP_INTn | N2 | input | 3.3-V LVTTL

##

USB
Name | Location | Direction | Standard
--- | --- | --- | ---
OTG_D[0] | Y25 | inout | 3.3-V LVTTL
OTG_D[1] | AA27 | inout | 3.3-V LVTTL
OTG_D[2] | Y26 | inout | 3.3-V LVTTL
OTG_D[3] | AA30 | inout | 3.3-V LVTTL
OTG_D[4] | AB29 | inout | 3.3-V LVTTL
OTG_D[5] | AA28 | inout | 3.3-V LVTTL
OTG_D[6] | Y31 | inout | 3.3-V LVTTL
OTG_D[7] | AA31 | inout | 3.3-V LVTTL
OTG_D[8] | Y32 | inout | 3.3-V LVTTL
OTG_D[9] | Y34 | inout | 3.3-V LVTTL
OTG_D[10] | AB31 | inout | 3.3-V LVTTL
OTG_D[11] | AA32 | inout | 3.3-V LVTTL
OTG_D[12] | AA33 | inout | 3.3-V LVTTL
OTG_D[13] | AD34 | inout | 3.3-V LVTTL
OTG_D[14] | AA34 | inout | 3.3-V LVTTL
OTG_D[15] | AC34 | inout | 3.3-V LVTTL
OTG_D[16] | AB30 | inout | 3.3-V LVTTL
OTG_D[17] | AB33 | inout | 3.3-V LVTTL
OTG_D[18] | AD33 | inout | 3.3-V LVTTL
OTG_D[19] | AB34 | inout | 3.3-V LVTTL
OTG_D[20] | AB32 | inout | 3.3-V LVTTL
OTG_D[21] | V24 | inout | 3.3-V LVTTL
OTG_D[22] | W26 | inout | 3.3-V LVTTL
OTG_D[23] | V25 | inout | 3.3-V LVTTL
OTG_D[24] | W30 | inout | 3.3-V LVTTL
OTG_D[25] | W27 | inout | 3.3-V LVTTL
OTG_D[26] | W31 | inout | 3.3-V LVTTL
OTG_D[27] | W24 | inout | 3.3-V LVTTL
OTG_D[28] | Y23 | inout | 3.3-V LVTTL
OTG_D[29] | Y29 | inout | 3.3-V LVTTL
OTG_D[30] | Y28 | inout | 3.3-V LVTTL
OTG_D[31] | AA29 | inout | 3.3-V LVTTL
OTG_A[1] | N32 | output | 3.3-V LVTTL
OTG_A[2] | L34 | output | 3.3-V LVTTL
OTG_A[3] | M31 | output | 3.3-V LVTTL
OTG_A[4] | N33 | output | 3.3-V LVTTL
OTG_A[5] | M33 | output | 3.3-V LVTTL
OTG_A[6] | M34 | output | 3.3-V LVTTL
OTG_A[7] | N34 | output | 3.3-V LVTTL
OTG_A[8] | N31 | output | 3.3-V LVTTL
OTG_A[9] | P34 | output | 3.3-V LVTTL
OTG_A[10] | P31 | output | 3.3-V LVTTL
OTG_A[11] | P32 | output | 3.3-V LVTTL
OTG_A[12] | R34 | output | 3.3-V LVTTL
OTG_A[13] | R33 | output | 3.3-V LVTTL
OTG_A[14] | R32 | output | 3.3-V LVTTL
OTG_A[15] | T32 | output | 3.3-V LVTTL
OTG_A[16] | U32 | output | 3.3-V LVTTL
OTG_A[17] | R31 | output | 3.3-V LVTTL
OTG_CS_n | P28 | output | 3.3-V LVTTL
OTG_WE_n | N29 | output | 3.3-V LVTTL
OTG_OE_n | N30 | output | 3.3-V LVTTL
OTG_HC_IRQ | P29 | input | 3.3-V LVTTL
OTG_DC_IRQ | R27 | input | 3.3-V LVTTL
OTG_RESET_n | T23 | output | 3.3-V LVTTL
OTG_HC_DREQ | R28 | input | 3.3-V LVTTL
OTG_HC_DACK | R25 | output | 3.3-V LVTTL
OTG_DC_DREQ | R26 | input | 3.3-V LVTTL
OTG_DC_DACK | R24 | output | 3.3-V LVTTL

##

SDCARD
Name | Location | Direction | Standard
--- | --- | --- | ---
SD_CMD | R10 | inout | 3.3-V LVTTL
SD_CLK | P8 | output | 3.3-V LVTTL
SD_DAT | P7 | inout | 3.3-V LVTTL
SD_WPn | N5 | input | 3.3-V LVTTL

##

Connector Name: GPIO0 (J13, GPIO 0)
Name | Location | Direction | Standard | Pin Index
--- | --- | --- | --- | ---
GPIO0_CLKINn0 | AE32 | inout | 3.3-V LVTTL | 1
GPIO0_D[0] | AL33 | inout | 3.3-V LVTTL | 2
GPIO0_CLKINp0 | AE31 | inout | 3.3-V LVTTL | 3
GPIO0_D[1] | AL32 | inout | 3.3-V LVTTL | 4
GPIO0_D[2] | AL34 | inout | 3.3-V LVTTL | 5
GPIO0_D[3] | AH31 | inout | 3.3-V LVTTL | 6
GPIO0_D[4] | AM34 | inout | 3.3-V LVTTL | 7
GPIO0_D[5] | AH30 | inout | 3.3-V LVTTL | 8
GPIO0_D[6] | AK34 | inout | 3.3-V LVTTL | 9
GPIO0_D[7] | AJ32 | inout | 3.3-V LVTTL | 10
GPIO0_D[8] | AK33 | inout | 3.3-V LVTTL | 13
GPIO0_D[9] | AJ31 | inout | 3.3-V LVTTL | 14
GPIO0_D[10] | AH34 | inout | 3.3-V LVTTL | 15
GPIO0_D[11] | AG32 | inout | 3.3-V LVTTL | 16
GPIO0_D[12] | AJ34 | inout | 3.3-V LVTTL | 17
GPIO0_D[13] | AG31 | inout | 3.3-V LVTTL | 18
GPIO0_CLKOUTn0 | AE19 | inout | 3.3-V LVTTL | 19
GPIO0_D[14] | AF32 | inout | 3.3-V LVTTL | 20
GPIO0_CLKOUTp0 | AD19 | inout | 3.3-V LVTTL | 21
GPIO0_D[15] | AF31 | inout | 3.3-V LVTTL | 22
GPIO0_D[16] | AP21 | inout | 3.3-V LVTTL | 23
GPIO0_D[17] | AG34 | inout | 3.3-V LVTTL | 24
GPIO0_D[18] | AN21 | inout | 3.3-V LVTTL | 25
GPIO0_D[19] | AH33 | inout | 3.3-V LVTTL | 26
GPIO0_D[20] | AL21 | inout | 3.3-V LVTTL | 27
GPIO0_D[21] | AP22 | inout | 3.3-V LVTTL | 28
GPIO0_D[22] | AK21 | inout | 3.3-V LVTTL | 31
GPIO0_D[23] | AN22 | inout | 3.3-V LVTTL | 32
GPIO0_D[24] | AP25 | inout | 3.3-V LVTTL | 33
GPIO0_D[25] | AP24 | inout | 3.3-V LVTTL | 34
GPIO0_D[26] | AN25 | inout | 3.3-V LVTTL | 35
GPIO0_D[27] | AN24 | inout | 3.3-V LVTTL | 36
GPIO0_D[28] | AM23 | inout | 3.3-V LVTTL | 37
GPIO0_D[29] | AG21 | inout | 3.3-V LVTTL | 38
GPIO0_D[30] | AL23 | inout | 3.3-V LVTTL | 39
GPIO0_D[31] | AF21 | inout | 3.3-V LVTTL | 40

##

Connector Name: GPIO1 (J14, GPIO 1)
Name | Location | Direction | Standard | Pin Index
--- | --- | --- | --- | ---
GPIO1_CLKINn1 | AP19 | inout | 3.3-V LVTTL | 1
GPIO1_D[0] | AC26 | inout | 3.3-V LVTTL | 2
GPIO1_CLKINp1 | AN19 | inout | 3.3-V LVTTL | 3
GPIO1_D[1] | AC25 | inout | 3.3-V LVTTL | 4
GPIO1_D[2] | AE28 | inout | 3.3-V LVTTL | 5
GPIO1_D[3] | AD27 | inout | 3.3-V LVTTL | 6
GPIO1_D[4] | AE27 | inout | 3.3-V LVTTL | 7
GPIO1_D[5] | AD26 | inout | 3.3-V LVTTL | 8
GPIO1_D[6] | AD29 | inout | 3.3-V LVTTL | 9
GPIO1_D[7] | AF29 | inout | 3.3-V LVTTL | 10
GPIO1_D[8] | AD28 | inout | 3.3-V LVTTL | 13
GPIO1_D[9] | AF28 | inout | 3.3-V LVTTL | 14
GPIO1_D[10] | AB27 | inout | 3.3-V LVTTL | 15
GPIO1_D[11] | AE30 | inout | 3.3-V LVTTL | 16
GPIO1_D[12] | AB26 | inout | 3.3-V LVTTL | 17
GPIO1_D[13] | AE29 | inout | 3.3-V LVTTL | 18
GPIO1_CLKOUTn1 | AE18 | inout | 3.3-V LVTTL | 19
GPIO1_D[14] | AB25 | inout | 3.3-V LVTTL | 20
GPIO1_CLKOUTp1 | AD18 | inout | 3.3-V LVTTL | 21
GPIO1_D[15] | AB24 | inout | 3.3-V LVTTL | 22
GPIO1_D[16] | AM21 | inout | 3.3-V LVTTL | 23
GPIO1_D[17] | AD31 | inout | 3.3-V LVTTL | 24
GPIO1_D[18] | AP20 | inout | 3.3-V LVTTL | 25
GPIO1_D[19] | AD30 | inout | 3.3-V LVTTL | 26
GPIO1_D[20] | AL22 | inout | 3.3-V LVTTL | 27
GPIO1_D[21] | AJ20 | inout | 3.3-V LVTTL | 28
GPIO1_D[22] | AM22 | inout | 3.3-V LVTTL | 31
GPIO1_D[23] | AJ21 | inout | 3.3-V LVTTL | 32
GPIO1_D[24] | AD21 | inout | 3.3-V LVTTL | 33
GPIO1_D[25] | AP26 | inout | 3.3-V LVTTL | 34
GPIO1_D[26] | AE20 | inout | 3.3-V LVTTL | 35
GPIO1_D[27] | AP23 | inout | 3.3-V LVTTL | 36
GPIO1_D[28] | AK24 | inout | 3.3-V LVTTL | 37
GPIO1_D[29] | AE22 | inout | 3.3-V LVTTL | 38
GPIO1_D[30] | AL25 | inout | 3.3-V LVTTL | 39
GPIO1_D[31] | AE21 | inout | 3.3-V LVTTL | 40

##

Connector Name: DDR2 (J9, DDR2 SO-DIMM)
Name | Location | Direction | Standard | Pin Index
--- | --- | --- | --- | ---
DDR2_DQ[4] | AE7 | inout | SSTL-18 Class I | 4
DDR2_DQ[0] | AM1 | inout | SSTL-18 Class I | 5
DDR2_DQ[5] | AE8 | inout | SSTL-18 Class I | 6
DDR2_DQ[1] | AM2 | inout | SSTL-18 Class I | 7
DDR2_DM[0] | AF5 | output | SSTL-18 Class I | 10
DDR2_DQS_n[0] | AJ3 | inout | SSTL-18 Class I | 11
DDR2_DQS_p[0] | AJ4 | inout | SSTL-18 Class I | 13
DDR2_DQ[6] | AC8 | inout | SSTL-18 Class I | 14
DDR2_DQ[7] | AC9 | inout | SSTL-18 Class I | 16
DDR2_DQ[2] | AL1 | inout | SSTL-18 Class I | 17
DDR2_DQ[3] | AL2 | inout | SSTL-18 Class I | 19
DDR2_DQ[12] | AE5 | inout | SSTL-18 Class I | 20
DDR2_DQ[13] | AE6 | inout | SSTL-18 Class I | 22
DDR2_DQ[8] | AG3 | inout | SSTL-18 Class I | 23
DDR2_DQ[9] | AG4 | inout | SSTL-18 Class I | 25
DDR2_DM[1] | AB10 | output | SSTL-18 Class I | 26
DDR2_DQS_n[1] | AK1 | inout | SSTL-18 Class I | 29
DDR2_CLK_p[0] | AE4 | inout | SSTL-18 Class I | 30
DDR2_DQS_p[1] | AJ2 | inout | SSTL-18 Class I | 31
DDR2_CLK_n[0] | AE3 | inout | SSTL-18 Class I | 32
DDR2_DQ[10] | AJ1 | inout | SSTL-18 Class I | 35
DDR2_DQ[14] | AD6 | inout | SSTL-18 Class I | 36
DDR2_DQ[11] | AH2 | inout | SSTL-18 Class I | 37
DDR2_DQ[15] | AD7 | inout | SSTL-18 Class I | 38
DDR2_DQ[16] | AF3 | inout | SSTL-18 Class I | 43
DDR2_DQ[20] | AC7 | inout | SSTL-18 Class I | 44
DDR2_DQ[17] | AF4 | inout | SSTL-18 Class I | 45
DDR2_DQ[21] | AB8 | inout | SSTL-18 Class I | 46
DDR2_DQS_n[2] | AH1 | inout | SSTL-18 Class I | 49
DDR2_DQS_p[2] | AG1 | inout | SSTL-18 Class I | 51
DDR2_DM[2] | AB9 | output | SSTL-18 Class I | 52
DDR2_DQ[18] | AF1 | inout | SSTL-18 Class I | 55
DDR2_DQ[22] | AC5 | inout | SSTL-18 Class I | 56
DDR2_DQ[19] | AF2 | inout | SSTL-18 Class I | 57
DDR2_DQ[23] | AC6 | inout | SSTL-18 Class I | 58
DDR2_DQ[24] | AJ15 | inout | SSTL-18 Class I | 61
DDR2_DQ[28] | AK15 | inout | SSTL-18 Class I | 62
DDR2_DQ[25] | AH15 | inout | SSTL-18 Class I | 63
DDR2_DQ[29] | AG15 | inout | SSTL-18 Class I | 64
DDR2_DM[3] | AN13 | output | SSTL-18 Class I | 67
DDR2_DQS_n[3] | AJ14 | inout | SSTL-18 Class I | 68
DDR2_DQS_p[3] | AH14 | inout | SSTL-18 Class I | 70
DDR2_DQ[26] | AP12 | inout | SSTL-18 Class I | 73
DDR2_DQ[30] | AP13 | inout | SSTL-18 Class I | 74
DDR2_DQ[27] | AN12 | inout | SSTL-18 Class I | 75
DDR2_DQ[31] | AM12 | inout | SSTL-18 Class I | 76
DDR2_CKE[0] | AF6 | output | SSTL-18 Class I | 79
DDR2_CKE[1] | AC11 | output | SSTL-18 Class I | 80
DDR2_A[15] | AA10 | output | SSTL-18 Class I | 84
DDR2_BA[2] | AP14 | output | SSTL-18 Class I | 85
DDR2_A[14] | AE15 | output | SSTL-18 Class I | 86
DDR2_A[12] | AM8 | output | SSTL-18 Class I | 89
DDR2_A[11] | AJ10 | output | SSTL-18 Class I | 90
DDR2_A[9] | AK7 | output | SSTL-18 Class I | 91
DDR2_A[7] | AM6 | output | SSTL-18 Class I | 92
DDR2_A[8] | AJ7 | output | SSTL-18 Class I | 93
DDR2_A[6] | AK6 | output | SSTL-18 Class I | 94
DDR2_A[5] | AM14 | output | SSTL-18 Class I | 97
DDR2_A[4] | AJ6 | output | SSTL-18 Class I | 98
DDR2_A[3] | AL14 | output | SSTL-18 Class I | 99
DDR2_A[2] | AF10 | output | SSTL-18 Class I | 100
DDR2_A[1] | AD12 | output | SSTL-18 Class I | 101
DDR2_A[0] | AE10 | output | SSTL-18 Class I | 102
DDR2_A[10] | AC12 | output | SSTL-18 Class I | 105
DDR2_BA[1] | AE12 | output | SSTL-18 Class I | 106
DDR2_BA[0] | AM17 | output | SSTL-18 Class I | 107
DDR2_RAS_n | AL13 | output | SSTL-18 Class I | 108
DDR2_WE_n | AL17 | output | SSTL-18 Class I | 109
DDR2_CS_n[0] | AM16 | output | SSTL-18 Class I | 110
DDR2_CAS_n | AD13 | output | SSTL-18 Class I | 113
DDR2_ODT[0] | AM15 | output | SSTL-18 Class I | 114
DDR2_CS_n[1] | AL16 | output | SSTL-18 Class I | 115
DDR2_A[13] | AL15 | output | SSTL-18 Class I | 116
DDR2_ODT[1] | AJ16 | output | SSTL-18 Class I | 119
DDR2_DQ[32] | AP10 | inout | SSTL-18 Class I | 123
DDR2_DQ[36] | AP11 | inout | SSTL-18 Class I | 124
DDR2_DQ[33] | AN10 | inout | SSTL-18 Class I | 125
DDR2_DQ[37] | AP9 | inout | SSTL-18 Class I | 126
DDR2_DQS_n[4] | AN9 | inout | SSTL-18 Class I | 129
DDR2_DM[4] | AF15 | output | SSTL-18 Class I | 130
DDR2_DQS_p[4] | AM9 | inout | SSTL-18 Class I | 131
DDR2_DQ[38] | AE14 | inout | SSTL-18 Class I | 134
DDR2_DQ[34] | AF14 | inout | SSTL-18 Class I | 135
DDR2_DQ[39] | AE13 | inout | SSTL-18 Class I | 136
DDR2_DQ[35] | AF13 | inout | SSTL-18 Class I | 137
DDR2_DQ[44] | AM11 | inout | SSTL-18 Class I | 140
DDR2_DQ[40] | AL12 | inout | SSTL-18 Class I | 141
DDR2_DQ[45] | AK10 | inout | SSTL-18 Class I | 142
DDR2_DQ[41] | AK12 | inout | SSTL-18 Class I | 143
DDR2_DQS_n[5] | AL11 | inout | SSTL-18 Class I | 146
DDR2_DM[5] | AP8 | output | SSTL-18 Class I | 147
DDR2_DQS_p[5] | AL10 | inout | SSTL-18 Class I | 148
DDR2_DQ[42] | AP7 | inout | SSTL-18 Class I | 151
DDR2_DQ[46] | AM7 | inout | SSTL-18 Class I | 152
DDR2_DQ[43] | AN7 | inout | SSTL-18 Class I | 153
DDR2_DQ[47] | AP6 | inout | SSTL-18 Class I | 154
DDR2_DQ[48] | AJ12 | inout | SSTL-18 Class I | 157
DDR2_DQ[52] | AJ13 | inout | SSTL-18 Class I | 158
DDR2_DQ[49] | AH12 | inout | SSTL-18 Class I | 159
DDR2_DQ[53] | AG12 | inout | SSTL-18 Class I | 160
DDR2_CLK_p[1] | AE11 | inout | SSTL-18 Class I | 164
DDR2_CLK_n[1] | AF11 | inout | SSTL-18 Class I | 166
DDR2_DQS_n[6] | AJ11 | inout | SSTL-18 Class I | 167
DDR2_DQS_p[6] | AH11 | inout | SSTL-18 Class I | 169
DDR2_DM[6] | AL8 | output | SSTL-18 Class I | 170
DDR2_DQ[50] | AL9 | inout | SSTL-18 Class I | 173
DDR2_DQ[54] | AJ9 | inout | SSTL-18 Class I | 174
DDR2_DQ[51] | AK9 | inout | SSTL-18 Class I | 175
DDR2_DQ[55] | AL7 | inout | SSTL-18 Class I | 176
DDR2_DQ[56] | AP4 | inout | SSTL-18 Class I | 179
DDR2_DQ[60] | AP5 | inout | SSTL-18 Class I | 180
DDR2_DQ[57] | AN4 | inout | SSTL-18 Class I | 181
DDR2_DQ[61] | AP2 | inout | SSTL-18 Class I | 182
DDR2_DM[7] | AN6 | output | SSTL-18 Class I | 185
DDR2_DQS_n[7] | AP3 | inout | SSTL-18 Class I | 186
DDR2_DQS_p[7] | AN3 | inout | SSTL-18 Class I | 188
DDR2_DQ[58] | AM5 | inout | SSTL-18 Class I | 189
DDR2_DQ[59] | AL5 | inout | SSTL-18 Class I | 191
DDR2_DQ[62] | AM4 | inout | SSTL-18 Class I | 192
DDR2_DQ[63] | AL4 | inout | SSTL-18 Class I | 194
DDR2_SDA | T9 | inout | 3.3-V LVTTL | 195
DDR2_SCL | T8 | output | 3.3-V LVTTL | 197
DDR2_SA[0] | U6 | output | 3.3-V LVTTL | 198
DDR2_SA[1] | T7 | output | 3.3-V LVTTL | 200

##

Connector Name: HSTCC (J5 HSTC-C TOP/J6, HSTC-C BOTTOM)
Connect to: CLR(Camera Link Receiver Board)
Name | Location | Direction | Standard | Pin Index
--- | --- | --- | --- | ---
CLR_RX_BASE[3] | L8 | input | 3.3-V LVTTL | 9
CLR_RX_BASE[4] | D2 | input | 3.3-V LVTTL | 10
CLR_RX_BASE[2] | L9 | input | 3.3-V LVTTL | 11
CLR_RX_BASE[5] | D3 | input | 3.3-V LVTTL | 12
CLR_RX_BASE[1] | M9 | input | 3.3-V LVTTL | 15
CLR_RX_BASE[6] | D1 | input | 3.3-V LVTTL | 16
CLR_RX_BASE[0] | M10 | input | 3.3-V LVTTL | 17
CLR_RX_BASE[7] | C1 | input | 3.3-V LVTTL | 18
CLR_RXCC[4] | K7 | output | 3.3-V LVTTL | 21
CLR_RX_BASE[8] | G4 | input | 3.3-V LVTTL | 22
CLR_RXCC[3] | K8 | output | 3.3-V LVTTL | 23
CLR_RX_BASE[9] | G5 | input | 3.3-V LVTTL | 24
CLR_RXCC[2] | J6 | output | 3.3-V LVTTL | 27
CLR_RX_BASE[10] | F3 | input | 3.3-V LVTTL | 28
CLR_RXCC[1] | J7 | output | 3.3-V LVTTL | 29
CLR_RX_BASE[11] | F4 | input | 3.3-V LVTTL | 30
CLR_RXCC_EN | N10 | output | 3.3-V LVTTL | 33
CLR_RX_BASE[12] | E1 | input | 3.3-V LVTTL | 34
CLR_RXSERTFG_EN | N11 | output | 3.3-V LVTTL | 35
CLR_RX_BASE[13] | E2 | input | 3.3-V LVTTL | 36
CLR_RXSERTFG | K5 | input | 3.3-V LVTTL | 39
CLR_RX_BASE[14] | H3 | input | 3.3-V LVTTL | 40
CLR_RXSERTC | K6 | output | 3.3-V LVTTL | 41
CLR_RX_BASE[15] | H4 | input | 3.3-V LVTTL | 42
CLR_RXSERTC_EN | N8 | output | 3.3-V LVTTL | 45
CLR_RX_BASE[16] | G1 | input | 3.3-V LVTTL | 46
CLR_RX_BASE[27] | N9 | input | 3.3-V LVTTL | 47
CLR_RX_BASE[17] | F1 | input | 3.3-V LVTTL | 48
CLR_RX_BASE[26] | L6 | input | 3.3-V LVTTL | 51
CLR_RX_BASE[18] | J3 | input | 3.3-V LVTTL | 52
CLR_RX_BASE[25] | L7 | input | 3.3-V LVTTL | 53
CLR_RX_BASE[19] | J4 | input | 3.3-V LVTTL | 54
CLR_RX_BASE[24] | L4 | input | 3.3-V LVTTL | 57
CLR_RX_BASE[20] | H1 | input | 3.3-V LVTTL | 58
CLR_RX_BASE[23] | L5 | input | 3.3-V LVTTL | 59
CLR_RX_BASE[21] | G2 | input | 3.3-V LVTTL | 60
CLR_RXCLK_BASE | A16 | input | 3.3-V LVTTL | 64
CLR_RXCLK_FULL | B16 | input | 3.3-V LVTTL | 66
CLR_RX_BASE[22] | A15 | input | 3.3-V LVTTL | 69
CLR_RX_FULL[3] | A14 | input | 3.3-V LVTTL | 70
CLR_RX_FULL[0] | C14 | input | 3.3-V LVTTL | 71
CLR_RX_FULL[4] | B14 | input | 3.3-V LVTTL | 72
CLR_RX_FULL[2] | F15 | input | 3.3-V LVTTL | 75
CLR_RX_FULL[5] | A13 | input | 3.3-V LVTTL | 76
CLR_RX_FULL[1] | D15 | input | 3.3-V LVTTL | 77
CLR_RX_FULL[6] | B13 | input | 3.3-V LVTTL | 78
CLR_RX2CC[4] | D14 | output | 3.3-V LVTTL | 81
CLR_RX_FULL[7] | E14 | input | 3.3-V LVTTL | 82
CLR_RX2CC[3] | E13 | output | 3.3-V LVTTL | 83
CLR_RX_FULL[8] | F14 | input | 3.3-V LVTTL | 84
CLR_RX2CC[2] | A12 | output | 3.3-V LVTTL | 87
CLR_RX_FULL[9] | A11 | input | 3.3-V LVTTL | 88
CLR_RX2CC[1] | A9 | output | 3.3-V LVTTL | 89
CLR_RX_FULL[10] | B11 | input | 3.3-V LVTTL | 90
CLR_RX2CC_EN | K15 | output | 3.3-V LVTTL | 93
CLR_RX_FULL[11] | A10 | input | 3.3-V LVTTL | 94
CLR_RX2SERTFG_EN | L14 | output | 3.3-V LVTTL | 95
CLR_RX_FULL[12] | B10 | input | 3.3-V LVTTL | 96
CLR_RX2SERTFG | K14 | input | 3.3-V LVTTL | 99
CLR_RX_FULL[13] | H14 | input | 3.3-V LVTTL | 100
CLR_RX2SERTC | K13 | output | 3.3-V LVTTL | 101
CLR_RX_FULL[20] | J14 | input | 3.3-V LVTTL | 102
CLR_RX2SERTC_EN | D13 | output | 3.3-V LVTTL | 105
CLR_RX_FULL[19] | C12 | input | 3.3-V LVTTL | 106
CLR_RX_FULL[21] | D10 | input | 3.3-V LVTTL | 107
CLR_RX_FULL[18] | D12 | input | 3.3-V LVTTL | 108
CLR_RX_FULL[27] | G13 | input | 3.3-V LVTTL | 111
CLR_RX_FULL[14] | C11 | input | 3.3-V LVTTL | 112
CLR_RX_FULL[26] | E11 | input | 3.3-V LVTTL | 113
CLR_RX_FULL[15] | D11 | input | 3.3-V LVTTL | 114
CLR_RX_FULL[24] | G12 | input | 3.3-V LVTTL | 117
CLR_RX_FULL[16] | F12 | input | 3.3-V LVTTL | 118
CLR_RX_FULL[25] | F11 | input | 3.3-V LVTTL | 119
CLR_RX_FULL[17] | F13 | input | 3.3-V LVTTL | 120
CLR_RXCLK_MEDIUM | A17 | input | 3.3-V LVTTL | 124
CLR_HSTC_SDA | T5 | inout | 3.3-V LVTTL | 131
CLR_HSTC_SCL | T4 | output | 3.3-V LVTTL | 132
CLR_RX_FULL[23] | A6 | input | 3.3-V LVTTL | 133
CLR_RX_MEDIUM[0] | A8 | input | 3.3-V LVTTL | 134
CLR_RX_FULL[22] | C7 | input | 3.3-V LVTTL | 135
CLR_RX_MEDIUM[1] | B8 | input | 3.3-V LVTTL | 136
CLR_RX_MEDIUM[2] | A7 | input | 3.3-V LVTTL | 138
CLR_RX_MEDIUM[3] | B7 | input | 3.3-V LVTTL | 140
CLR_RX_MEDIUM[4] | C9 | input | 3.3-V LVTTL | 142
CLR_RX_MEDIUM[5] | D9 | input | 3.3-V LVTTL | 144
CLR_RX_MEDIUM[6] | A4 | input | 3.3-V LVTTL | 146
CLR_RX_MEDIUM[7] | B4 | input | 3.3-V LVTTL | 148
CLR_RX_MEDIUM[8] | A2 | input | 3.3-V LVTTL | 150
CLR_RX_MEDIUM[9] | B2 | input | 3.3-V LVTTL | 152
CLR_RX_MEDIUM[10] | G11 | input | 3.3-V LVTTL | 154
CLR_RX_MEDIUM[11] | H11 | input | 3.3-V LVTTL | 156
CLR_RX_MEDIUM[12] | B5 | input | 3.3-V LVTTL | 158
CLR_RX_MEDIUM[13] | C5 | input | 3.3-V LVTTL | 160
CLR_RX_MEDIUM[14] | C3 | input | 3.3-V LVTTL | 162
CLR_RX_MEDIUM[15] | C4 | input | 3.3-V LVTTL | 164
CLR_RX_MEDIUM[16] | C16 | input | 3.3-V LVTTL | 166
CLR_RX_MEDIUM[17] | D16 | input | 3.3-V LVTTL | 168
CLR_RX_MEDIUM[18] | K11 | input | 3.3-V LVTTL | 170
CLR_RX_MEDIUM[26] | K12 | input | 3.3-V LVTTL | 172
CLR_RX_MEDIUM[25] | C17 | input | 3.3-V LVTTL | 173
CLR_RX_MEDIUM[19] | E16 | input | 3.3-V LVTTL | 174
CLR_RX_MEDIUM[24] | C15 | input | 3.3-V LVTTL | 175
CLR_RX_MEDIUM[20] | F16 | input | 3.3-V LVTTL | 176
CLR_RX_MEDIUM[22] | D17 | input | 3.3-V LVTTL | 177
CLR_RX_MEDIUM[21] | J16 | input | 3.3-V LVTTL | 178
CLR_RX_MEDIUM[23] | E17 | input | 3.3-V LVTTL | 179
CLR_RX_MEDIUM[27] | J15 | input | 3.3-V LVTTL | 180

##

Connector Name: HSTCD (J7, HSTC-D TOP/J8, HSTC-D BOTTOM)
Name | Location | Direction | Standard | Pin Index
--- | --- | --- | --- | ---
HSTCD_CLKOUT_n[0] | L20 | inout | 3.3-V LVTTL | 3
HSTCD_CLKIN_n[0] | J34 | inout | 3.3-V LVTTL | 4
HSTCD_CLKOUT_p[0] | L19 | inout | 3.3-V LVTTL | 5
HSTCD_CLKIN_p[0] | J33 | inout | 3.3-V LVTTL | 6
HSTCD_TX_n[0] | J30 | inout | 3.3-V LVTTL | 9
HSTCD_RX_n[0] | F32 | inout | 3.3-V LVTTL | 10
HSTCD_TX_p[0] | J29 | inout | 3.3-V LVTTL | 11
HSTCD_RX_p[0] | F31 | inout | 3.3-V LVTTL | 12
HSTCD_TX_n[1] | K28 | inout | 3.3-V LVTTL | 15
HSTCD_RX_n[1] | C34 | inout | 3.3-V LVTTL | 16
HSTCD_TX_p[1] | K27 | inout | 3.3-V LVTTL | 17
HSTCD_RX_p[1] | C33 | inout | 3.3-V LVTTL | 18
HSTCD_TX_n[2] | N25 | inout | 3.3-V LVTTL | 21
HSTCD_RX_n[2] | H32 | inout | 3.3-V LVTTL | 22
HSTCD_TX_p[2] | M24 | inout | 3.3-V LVTTL | 23
HSTCD_RX_p[2] | H31 | inout | 3.3-V LVTTL | 24
HSTCD_TX_n[3] | M27 | inout | 3.3-V LVTTL | 27
HSTCD_RX_n[3] | D34 | inout | 3.3-V LVTTL | 28
HSTCD_TX_p[3] | M26 | inout | 3.3-V LVTTL | 29
HSTCD_RX_p[3] | D33 | inout | 3.3-V LVTTL | 30
HSTCD_TX_n[4] | K30 | inout | 3.3-V LVTTL | 33
HSTCD_RX_n[4] | J32 | inout | 3.3-V LVTTL | 34
HSTCD_TX_p[4] | K29 | inout | 3.3-V LVTTL | 35
HSTCD_RX_p[4] | J31 | inout | 3.3-V LVTTL | 36
HSTCD_TX_n[5] | L29 | inout | 3.3-V LVTTL | 39
HSTCD_RX_n[5] | E34 | inout | 3.3-V LVTTL | 40
HSTCD_TX_p[5] | L28 | inout | 3.3-V LVTTL | 41
HSTCD_RX_p[5] | F33 | inout | 3.3-V LVTTL | 42
HSTCD_TX_n[6] | M28 | inout | 3.3-V LVTTL | 45
HSTCD_RX_n[6] | F34 | inout | 3.3-V LVTTL | 46
HSTCD_TX_p[6] | N27 | inout | 3.3-V LVTTL | 47
HSTCD_RX_p[6] | G33 | inout | 3.3-V LVTTL | 48
HSTCD_TX_n[7] | N26 | inout | 3.3-V LVTTL | 51
HSTCD_RX_n[7] | K32 | inout | 3.3-V LVTTL | 52
HSTCD_TX_p[7] | P25 | inout | 3.3-V LVTTL | 53
HSTCD_RX_p[7] | K31 | inout | 3.3-V LVTTL | 54
HSTCD_TX_n[8] | L32 | inout | 3.3-V LVTTL | 57
HSTCD_RX_n[8] | G34 | inout | 3.3-V LVTTL | 58
HSTCD_TX_p[8] | L31 | inout | 3.3-V LVTTL | 59
HSTCD_RX_p[8] | H34 | inout | 3.3-V LVTTL | 60
HSTCD_CLKOUT_n[1] | J19 | inout | 3.3-V LVTTL | 63
HSTCD_CLKIN_n[1] | A20 | inout | 3.3-V LVTTL | 64
HSTCD_CLKOUT_p[1] | K19 | inout | 3.3-V LVTTL | 65
HSTCD_CLKIN_p[1] | B20 | inout | 3.3-V LVTTL | 66
HSTCD_TX_n[9] | H20 | inout | 3.3-V LVTTL | 69
HSTCD_RX_n[9] | F20 | inout | 3.3-V LVTTL | 70
HSTCD_TX_p[9] | E20 | inout | 3.3-V LVTTL | 71
HSTCD_RX_p[9] | G20 | inout | 3.3-V LVTTL | 72
HSTCD_TX_n[10] | A21 | inout | 3.3-V LVTTL | 75
HSTCD_RX_n[10] | F21 | inout | 3.3-V LVTTL | 76
HSTCD_TX_p[10] | A22 | inout | 3.3-V LVTTL | 77
HSTCD_RX_p[10] | G21 | inout | 3.3-V LVTTL | 78
HSTCD_TX_n[11] | C23 | inout | 3.3-V LVTTL | 81
HSTCD_RX_n[11] | A23 | inout | 3.3-V LVTTL | 82
HSTCD_TX_p[11] | B22 | inout | 3.3-V LVTTL | 83
HSTCD_RX_p[11] | B23 | inout | 3.3-V LVTTL | 84
HSTCD_TX_n[12] | A26 | inout | 3.3-V LVTTL | 87
HSTCD_RX_n[12] | A25 | inout | 3.3-V LVTTL | 88
HSTCD_TX_p[12] | A24 | inout | 3.3-V LVTTL | 89
HSTCD_RX_p[12] | B25 | inout | 3.3-V LVTTL | 90
HSTCD_TX_n[13] | J20 | inout | 3.3-V LVTTL | 93
HSTCD_RX_n[13] | B26 | inout | 3.3-V LVTTL | 94
HSTCD_TX_p[13] | K20 | inout | 3.3-V LVTTL | 95
HSTCD_RX_p[13] | C26 | inout | 3.3-V LVTTL | 96
HSTCD_TX_n[14] | K22 | inout | 3.3-V LVTTL | 99
HSTCD_RX_n[14] | J21 | inout | 3.3-V LVTTL | 100
HSTCD_TX_p[14] | K21 | inout | 3.3-V LVTTL | 101
HSTCD_RX_p[14] | J22 | inout | 3.3-V LVTTL | 102
HSTCD_TX_n[15] | E25 | inout | 3.3-V LVTTL | 105
HSTCD_RX_n[15] | D24 | inout | 3.3-V LVTTL | 106
HSTCD_TX_p[15] | C24 | inout | 3.3-V LVTTL | 107
HSTCD_RX_p[15] | D25 | inout | 3.3-V LVTTL | 108
HSTCD_TX_n[16] | C27 | inout | 3.3-V LVTTL | 111
HSTCD_RX_n[16] | D23 | inout | 3.3-V LVTTL | 112
HSTCD_TX_p[16] | A27 | inout | 3.3-V LVTTL | 113
HSTCD_RX_p[16] | E23 | inout | 3.3-V LVTTL | 114
HSTCD_TX_n[17] | A29 | inout | 3.3-V LVTTL | 117
HSTCD_RX_n[17] | A28 | inout | 3.3-V LVTTL | 118
HSTCD_TX_p[17] | C28 | inout | 3.3-V LVTTL | 119
HSTCD_RX_p[17] | B28 | inout | 3.3-V LVTTL | 120
HSTCD_CLKOUT_2 | M29 | inout | 3.3-V LVTTL | 123
HSTCD_CLKIN_2 | A19 | inout | 3.3-V LVTTL | 124
HSTCD_SDA | R30 | inout | 3.3-V LVTTL | 131
HSTCD_SCL | R29 | output | 3.3-V LVTTL | 132
HSTCD_TX_n[18] | H23 | inout | 3.3-V LVTTL | 133
HSTCD_RX_n[18] | F23 | inout | 3.3-V LVTTL | 134
HSTCD_TX_p[18] | F22 | inout | 3.3-V LVTTL | 135
HSTCD_RX_p[18] | G23 | inout | 3.3-V LVTTL | 136
HSTCD_TX_n[19] | D27 | inout | 3.3-V LVTTL | 137
HSTCD_RX_n[19] | F24 | inout | 3.3-V LVTTL | 138
HSTCD_TX_p[19] | F25 | inout | 3.3-V LVTTL | 139
HSTCD_RX_p[19] | G24 | inout | 3.3-V LVTTL | 140
HSTCD_TX_n[20] | D28 | inout | 3.3-V LVTTL | 141
HSTCD_RX_n[20] | D26 | inout | 3.3-V LVTTL | 142
HSTCD_TX_p[20] | F26 | inout | 3.3-V LVTTL | 143
HSTCD_RX_p[20] | E26 | inout | 3.3-V LVTTL | 144
HSTCD_TX_n[21] | A33 | inout | 3.3-V LVTTL | 145
HSTCD_RX_n[21] | A31 | inout | 3.3-V LVTTL | 146
HSTCD_TX_p[21] | A30 | inout | 3.3-V LVTTL | 147
HSTCD_RX_p[21] | B31 | inout | 3.3-V LVTTL | 148
HSTCD_TX_n[22] | B29 | inout | 3.3-V LVTTL | 149
HSTCD_RX_n[22] | A32 | inout | 3.3-V LVTTL | 150
HSTCD_TX_p[22] | C29 | inout | 3.3-V LVTTL | 151
HSTCD_RX_p[22] | B32 | inout | 3.3-V LVTTL | 152
HSTCD_TX_n[23] | D31 | inout | 3.3-V LVTTL | 153
HSTCD_RX_n[23] | C30 | inout | 3.3-V LVTTL | 154
HSTCD_TX_p[23] | C31 | inout | 3.3-V LVTTL | 155
HSTCD_RX_p[23] | D30 | inout | 3.3-V LVTTL | 156
HSTCD_TX_n[24] | G27 | inout | 3.3-V LVTTL | 157
HSTCD_RX_n[24] | E28 | inout | 3.3-V LVTTL | 158
HSTCD_TX_p[24] | F27 | inout | 3.3-V LVTTL | 159
HSTCD_RX_p[24] | F28 | inout | 3.3-V LVTTL | 160
HSTCD_TX_n[25] | K24 | inout | 3.3-V LVTTL | 161
HSTCD_RX_n[25] | E29 | inout | 3.3-V LVTTL | 162
HSTCD_TX_p[25] | J24 | inout | 3.3-V LVTTL | 163
HSTCD_RX_p[25] | F29 | inout | 3.3-V LVTTL | 164
HSTCD_TX_n[26] | K25 | inout | 3.3-V LVTTL | 165
HSTCD_RX_n[26] | C21 | inout | 3.3-V LVTTL | 166
HSTCD_TX_p[26] | J25 | inout | 3.3-V LVTTL | 167
HSTCD_RX_p[26] | D21 | inout | 3.3-V LVTTL | 168
HSTCD_TX_n[27] | K23 | inout | 3.3-V LVTTL | 169
HSTCD_RX_n[27] | L23 | inout | 3.3-V LVTTL | 170
HSTCD_TX_p[27] | L22 | inout | 3.3-V LVTTL | 171
HSTCD_RX_p[27] | M23 | inout | 3.3-V LVTTL | 172
HSTCD_TX_n[28] | E22 | inout | 3.3-V LVTTL | 173
HSTCD_RX_n[28] | C18 | inout | 3.3-V LVTTL | 174
HSTCD_TX_p[28] | D22 | inout | 3.3-V LVTTL | 175
HSTCD_RX_p[28] | D18 | inout | 3.3-V LVTTL | 176
HSTCD_TX_n[29] | D20 | inout | 3.3-V LVTTL | 177
HSTCD_RX_n[29] | E19 | inout | 3.3-V LVTTL | 178
HSTCD_TX_p[29] | C20 | inout | 3.3-V LVTTL | 179
HSTCD_RX_p[29] | F19 | inout | 3.3-V LVTTL | 180