# Generation Report - NCO v11.0

Entity Name | lpm_nco10_st
Variation Name | lpm_nco10
Variation HDL | Verilog HDL
Output Directory | D:\SVN\tr4\daughter_card\Tr4_ADA\V

## File Summary

The MegaWizard interface is creating the following files in the output directory:

File | Description
--- | ---
lpm_nco10.v | A MegaCore® function variation file, which defines a Verilog HDL top-level description of the custom MegaCore function. Instantiate the entity defined by this file inside of your design. Include this file when compiling your design in the Quartus II software.
lpm_nco10_bb.v | Verilog HDL black-box file for the MegaCore function variation. Use this file when using a third-party EDA tool to synthesize your design.
lpm_nco10.bsf | Quartus® II symbol file for the MegaCore function variation. You can use this file in the Quartus II block diagram editor.
lpm_nco10_st.v | Generated NCO synthesizable netlist. This file is required for Quartus II synthesis. It will be added to your Quartus II project
lpm_nco10.vo | Verilog HDL IP Functional Simulation model
lpm_nco10_tb.v | Verilog HDL Testbench
lpm_nco10_vo_msim.tcl | ModelSim TCL Script to run the Verilog HDL IP Functional Simulation model and generated Verilog HDL testbench in the ModelSim simulation software
lpm_nco10_wave.do | ModelSim Waveform File
lpm_nco10_model.m | MATLAB m-file describing a MATLAB bit-accurate model.
lpm_nco10_tb.m | MATLAB Testbench
lpm_nco10_sin_f.hex | Intel Hex-format ROM initialization file.
lpm_nco10_cos_f.hex | Intel Hex-format ROM initialization file.
lpm_nco10_sin_c.hex | Intel Hex-format ROM initialization file.
lpm_nco10_cos_c.hex | Intel Hex-format ROM initialization file.
lpm_nco10.vec | Quartus II Vector File.
lpm_nco10_nativelink.tcl | A Tcl script that can be used to assign NativeLink simulation testbench settings to the Quartus II project
lpm_nco10.qip | Contains Quartus II project information for your MegaCore function variation.
lpm_nco10.html | The MegaCore function report file.

## MegaCore Function Variation File Ports

Name | Direction | Width
--- | --- | ---
phi_inc_i | INPUT | 32
fsin_o | OUTPUT | 14
fcos_o | OUTPUT | 14
clk | INPUT | 1
reset_n | INPUT | 1
clken | INPUT | 1
out_valid | OUTPUT | 1